{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["SAE # Thread Sizes"]
[]
["SAE No","Nominal Tube Size OD”","Thread Size”","TPI","OD mm","Pitch Dia E”","E mm","NPT Size”"]
[2,0.125,0.3125,24,{"$f":"C4*25.4","v":7.9375},{"$f":"C4-(0.64952/D4)","v":0.28543666666666667},{"$f":"F4*25.4","v":7.2500913333333328},"1/8’’ –  27"]
[3,0.1875,0.375,24,{"$f":"C5*25.4","v":9.5249999999999986},{"$f":"C5-(0.64952/D5)","v":0.34793666666666667},{"$f":"F5*25.4","v":8.8375913333333322}]
[4,0.25,0.4375,20,11.112499999999999,{"$f":"C6-(0.64952/D6)","v":0.405024},10.2876096,"1/4’’ – 18"]
[5,0.3125,0.5,20,12.7,{"$f":"C7-(0.64952/D7)","v":0.467524},11.8751096]
[6,0.375,0.5625,18,14.2875,{"$f":"C8-(0.64952/D8)","v":0.52641555555555553},13.37095511111111,"3/8’’ – 18"]
[8,0.5,0.75,16,19.049999999999997,{"$f":"C9-(0.64952/D9)","v":0.70940499999999995},18.018886999999999,"1/2’’ – 14"]
[10,0.625,0.875,14,22.224999999999998,{"$f":"C10-(0.64952/D10)","v":0.82860571428571428},21.04658514285714]
[12,0.75,1.0625,12,26.987499999999997,{"$f":"C11-(0.64952/D11)","v":1.0083733333333333},25.612682666666664,"3/4’’ – 14"]
[14,0.875,1.1875,12,30.162499999999998,{"$f":"C12-(0.64952/D12)","v":1.1333733333333333},28.787682666666665]
[16,1,1.3125,12,33.337499999999999,{"$f":"C13-(0.64952/D13)","v":1.2583733333333333},31.962682666666666,"1’’– 11.5"]
[20,1.25,1.625,12,41.274999999999999,{"$f":"C14-(0.64952/D14)","v":1.5708733333333333},39.900182666666666,"1 1/4’’– 11.5"]
[24,1.5,1.875,12,47.625,{"$f":"C15-(0.64952/D15)","v":1.8208733333333333},46.250182666666667,"1 1/2’’– 11.5"]
[32,2,2.5,12,63.5,{"$f":"C16-(0.64952/D16)","v":2.4458733333333331},62.12518266666666,"2’’– 11.5"]
[]
[null,"E=D-(0.64952/n)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}