customize

# Design Rule Verification Report

Date | : | 18/03/2013
Time | : | 09:15:27
Elapsed Time | : | 00:00:05
Filename | : | C:\Altium-Client\Agrigel\3-General\Flow-Controller\Flow-Controller.PcbDoc
Warnings | : | 0
Rule Violations | : | 0

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Hole Size Constraint (Min=9.842mil) (Max=196.85mil) (All) | 0
Component Clearance Constraint ( Horizontal Gap = 0mil, Vertical Gap = 1mil ) (All),(All) | 0
Routing Via (MinHoleWidth=11.811mil) (MaxHoleWidth=11.811mil) (PreferredHoleWidth=11.811mil) (MinWidth=27.559mil) (MaxWidth=27.559mil) (PreferedWidth=27.559mil) (All) | 0
Width Constraint (Min=7.874mil) (Max=78.74mil) (Preferred=7.874mil) (All) | 0
Power Plane Connect Rule(Relief Connect )(Expansion=20mil) (Conductor Width=10mil) (Air Gap=10mil) (Entries=4) (All) | 0
Clearance Constraint (Gap=6.693mil) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Width Constraint (Min=11.811mil) (Max=39.37mil) (Preferred=19.685mil) (InNetClass('Power')) | 0
Width Constraint (Min=19.685mil) (Max=59.055mil) (Preferred=39.37mil) (InNetClass('High Power')) | 0
Short-Circuit Constraint (Allowed=Yes) ((InComponent('LK1'))),(All) | 0
Short-Circuit Constraint (Allowed=Yes) ((InComponent('LK2'))),(All) | 0
Short-Circuit Constraint (Allowed=Yes) ((InComponent('LK3'))),(All) | 0
Total | 0