{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Slave ID Programmer Board (Bill"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Slave ID Programmer Board (Bill","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Report File:","C:\\Electronics\\Flow Control Board\\Slave ID Programmer\\Slave ID Programmer Board (Bill Of Materials).csv"]
["Report Written:","Tuesday, December 20, 2016"]
["Project Path:","C:\\Electronics\\Flow Control Board\\Slave ID Programmer\\Slave ID Programmer.prj"]
["Design Path:","C:\\Electronics\\Flow Control Board\\Slave ID Programmer\\Slave ID Programmer Board.pcb"]
["Design Title:"]
["Created:","2016-10-19T20:33:57"]
["Last Saved:","2016-12-20T19:41:01"]
["Editing Time:","305 min"]
["Units:","mm (precision 2)"]
[]
["Bill of Materials generated with DesignSpark PCB - www.DesignSpark.com/pcb"]
["--------------------------------------------------------------------------"]
[]
[]
["Ref Name","Qty","Component","Value","Package","Manufacturer","MPN","RS Part Number","Other Part Number","Description"]
["PL2",1,"CONN_SIL_2",null,"2 SIL",null,null,"681-3007",null,"2 way Pin Header"]
["PL1",1,"CON_SOCK_90Deg_7",null,"7 SIL","SULLINS","PPPC071LGBN-RC",null,"S5482-ND DigiKey","Female Header 90deg 7 way"]
["SW1",1,"DIP SW-6",null,"SWDIP12_300X138P100","TE","1825002-9","718-2102",null,"DIP switch,PCB,SPST,6 pos,flush slide"]
["LED1",1,"LED 3 TH Green",null,"LED_TLH","Vishay","TLHG4405",7082759,null,"LED Uni-Color Green"]
["LED2",1,"LED 3 TH Red",null,"LED_TLH","Vishay","TLHG4405","872-3149",null,"LED Uni-Color Red"]
[1,1,"RES TH 0.25W 5% 180R","180R","Res TH 04",null,null,"135-803",null,"Resistor, 180R 5% 0.25W, T H"]
[4,1,"RES TH 0.25W 5% 180R","180R","Res TH 04",null,null,"135-803",null,"Resistor, 180R 5% 0.25W, T H"]
[2,1,"RES TH 0.25W 5% 390R","390R","Res TH 04",null,null,"707-7634",null,"Resistor, 390R 5% 0.25W, T H"]
[5,1,"RES TH 0.25W 5% 390R","390R","Res TH 04",null,null,"707-7634",null,"Resistor, 390R 5% 0.25W, T H"]
[3,1,"RES TH 0.25W 5% 680R","680R","Res TH 04",null,null,"707-7656",null,"Resistor, 680R 5% 0.25W, T H"]
[6,1,"RES TH 0.25W 5% 680R","680R","Res TH 04",null,null,"707-7656",null,"Resistor, 680R 5% 0.25W, T H"]