{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Item Number","Title","Document Number","Quantity"]
[1,"FH Die Plate","446 x 596 x 96",1]
[2,"MH Die Plate","446 x 596 x 46",1]
[3,"Support Plate",56,1]
[4,"Ejector Plate Top",20,1]
[5,"Ejector Plate Bottom",26,1]
[6,"Riser",106,2]
[7,"MH Clamping Plate",36,1]
[8,"FH Clamping Plate",36,1]
[9,"Sprue Bush","Dia 18 - 55 long",1]
[10,"Locating Ring","LR-125",1]
[11,"Locating Bush",96,4]
[12,"Locating Pin","46-96",4]
[]
[13,"Angle Pin","D14 - 80",4]
[14,"Sleeve Ejector Pin","OD 6 - ID 4 x 200",4]
[15,"Ejector Pin","D 4 x 250",4]
[16,"Ejector Pin","D 3.5 x 200",12]
[17,"Ejector Pin","D 6 x 250",1]
[18,"Ejector Pin","D 10 x 200",8]
[19,"Ejector Pin","D 4 x 100",8]
[20,"Ejector Pin","D20 x 100"]
[]
[21,"Took Steel Blocks"]
[22,"SLIDES","270 x 64 x 64",2]
[23,"Insert","280 x 90 x 51",1]
[24,"RAILS","82 x 21 x 20",4]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}