{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Shut Off Board 01 (Bill Of Mate"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Shut Off Board 01 (Bill Of Mate","index":0,"n_rows":48,"n_cols":13,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
["Report File:","C:\\Electronics\\Shut Off Board\\Shut Off Board 01\\Shut Off Board 01 (Bill Of Materials).csv"]
["Report Written:","Tuesday, August 09, 2016"]
["Project Path:","C:\\Electronics\\Shut Off Board\\Shut Off Board 01\\Shut Off Board 01.prj"]
["Design Path:","C:\\Electronics\\Shut Off Board\\Shut Off Board 01\\Shut Off Board 01.pcb"]
["Design Title:"]
["Created:","2016-06-17T11:13:00"]
["Last Saved:","2016-08-09T10:19:33"]
["Editing Time:","3677 min"]
["Units:","mm (precision 2)"]
[]
["Bill of Materials generated with DesignSpark PCB - www.DesignSpark.com/pcb"]
["--------------------------------------------------------------------------"]
[]
[]
["Ref Name","Qty","Component","Value","Package","Manufacturer","MPN","RS Part Number","Other Part Number","Description"]
[11,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[6,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[8,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[10,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[3,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[4,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
[1,1,"1K","1K","RES0603_CRG_TYCO-L",null,null,2132266,null,"CRG0603 SMT chip resistor,1K 1% 0.1W"]
["J2",1,"3 Pin ST 5",null,"3 Con ST 5",null,null,"361-7673",null,"3 way Screw Terminal,5mm pitch"]
["J1",1,"3 Pin ST 5",null,"3 Con ST 5",null,null,"361-7673",null,"3 way Screw Terminal,5mm pitch"]
[7,1,"3K3",null,"RES0603_CRG_TYCO-L",null,null,2132339,null,"CRG0603 SMT chip resistor,3K3 1% 0.1W"]
[2,1,"4K7",null,"RES0603_CRG_TYCO-L",null,null,2132367,null,"CRG0603 SMT chip resistor,4K7 1% 0.1W"]
[9,1,"10k",null,"RES0603",null,null,"804-8921",null,"0603 10K Res"]
[5,1,"10k",null,"RES0603",null,null,"804-8921",null,"0603 10K Res"]
["C9",1,"10nF",null,"CAP_C0603-L",null,null,"904-0101",null,"Cap 10nF 50V 0603"]
["C5",1,"10uF",null,"CAP_C0603-L",null,null,"815-1355",null,"Cap 10uF 0603"]
["C3",1,"22nF",null,"CAP_C0603-L",null,null,"391-195",null,"Cap 22nF"]
["C8",1,"100nF",null,"CAP_C0603",null,null,"698-3260",null,"Cap 100nF 50v 0603"]
["C6",1,"100nF",null,"CAP_C0603",null,null,"698-3260",null,"Cap 100nF 50v 0603"]
["C4",1,"100nF",null,"CAP_C0603",null,null,"698-3260",null,"Cap 100nF 50v 0603"]
["C7",1,"100uF 35v AD10","100uF","PCAP 10x10",null,null,"520-2188",null,"Al cap, WG Series,SMT,35V,100F"]
["C2",1,"220pF",null,"CAP_C0603-L",null,null,"869-1938",null,"Cap 220pF"]
["C1",1,"470uF 25v D10","470uF","PCAP 10x10",null,"UCD1E471MNL1GS","715-1293",null,"Capacitor Aluminium SMT 470uF 25V"]
["PL1",1,"CONN_SIL_3",null,"3 SIL",null,null,"681-3007",null,"4 way Pin Header"]
["PL2",1,"CONN_SIL_7",null,"7 SIL",null,null,"681-3007",null,"7 way Pin Header"]
["D3",1,"ES3J",null,"DO-214AB","Fairchild Semiconductor","ES3J","761-3619",null,"Diode Switching 600V 3A DO214AB"]
["FS1",1,"FUSE HOLDER FLR","12V","SMTFuse 5x20","Schurter",null,"410-7672",null,"FUSE HOLDER"]
["LED1",1,"Led SMD0805 Green",null,"LED_PLCC_VSMB-L",null,null,"888-6304",null,"LED Green 0805"]
["LED2",1,"Led SMD0805 Yellow",null,"LED_SM 0805",null,null,"888-6316",null,"LED Yellow 0805"]
["U2",1,"PIC12F1840-I/SN",null,"SOIC8-N_MC",null,null,"889-5553",null,"8 bit PIC"]
["U1",1,"Reg-L5973D",null,"HSOP8-L","STMicroelectronics","L5973D",380034,null,"Switching Reg,2.5A,4-36Vin,HSOP8"]
["L1",1,"SDR0805-33uH","33uH","USER",null,"SDR0805-330KL","736-1286",null,"INDUCTOR POWER"]
["D2",1,"SMCJ26A",null,"DO-214AB","Vishay","SMCJ26A-E3/57T","631-1148",null,"Diode Uni-Directional"]
["D1",1,"SMS2100",null,"DO-213AB","Electrocomp",3291,null,3291,"Diod Schottky-Rectifiers",null,null,"SSA210 can be used"]