{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Shut Off Distribution Board (Bi"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Shut Off Distribution Board (Bi","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Report File:","C:\\Electronics\\Shut Off Board\\Shut Off Distribution Board\\Shut Off Distribution Board (Bill Of Materials).csv"]
["Report Written:","Wednesday, August 10, 2016"]
["Project Path:","C:\\Electronics\\Shut Off Board\\Shut Off Distribution Board\\Shut Off Distribution Board.prj"]
["Design Path:","C:\\Electronics\\Shut Off Board\\Shut Off Distribution Board\\Shut Off Distribution Board.pcb"]
["Design Title:"]
["Created:","2016-07-22T14:38:55"]
["Last Saved:","2016-08-10T11:26:19"]
["Editing Time:","492 min"]
["Units:","mm (precision 2)"]
[]
["Bill of Materials generated with DesignSpark PCB - www.DesignSpark.com/pcb"]
["--------------------------------------------------------------------------"]
[]
[]
["Ref Name","Qty","Component","Value","Package","Manufacturer","MPN","RS Part Number","Other Part Number","Description"]
["J5",1,"2 Pin ST 5",null,"2 Con ST 5",null,null,"361-7667",null,"2 way Screw Terminal,5mm pitch"]
["J6",1,"2 Pin ST 5",null,"2 Con ST 5",null,null,"361-7667",null,"2 way Screw Terminal,5mm pitch"]
["J1",1,"3 Pin ST 5",null,"3 Con ST 5",null,null,"361-7673",null,"3 way Screw Terminal,5mm pitch"]
["J2",1,"3 Pin ST 5",null,"3 Con ST 5",null,null,"361-7673",null,"3 way Screw Terminal,5mm pitch"]
["J3",1,"3 Pin ST 5",null,"3 Con ST 5",null,null,"361-7673",null,"3 way Screw Terminal,5mm pitch"]
["LED1",1,"LED 3 TH Green",null,"LED_TLH","Vishay","TLHG4405",7082759,null,"LED Uni-Color Green"]
["LED2",1,"LED 3 TH Yellow",null,"LED_TLH","Vishay","TLHY4405","708-2771",null,"LED Uni-Color Yellow"]
[1,1,"RES TH 0.25W 5% 1K","1.0K","Res TH 04",null,null,null,null,"Resistor TH 1K"]
[2,1,"RES TH 0.25W 5% 1K","1.0K","Res TH 04",null,null,null,null,"Resistor TH 1K"]